* Setup the feedback loop with a threshold of 27 (that was the room temperature)
* variation of +- 1 degree for high(28) and the low(26) temperature values.
* Changed the rc file to start the BMP and the GPIO services as part of the startup process.
* Both the BMP and GPIO support IPC and is used it to communicate with it.

  
  
  
